###Project Name
project name = Anyka

###Devie Number
device channel = 3

###planform name
planform name = RTOS

###COM
com bOpen = 0
com base = 1
com count = 1
com baud rate = 38400

path producer = ./producer_37xx.bin
path nandboot = ./Spiboot_37XX.bin

producer run addr = 0x30000000

chip type = AK_37XX
chip uboot = 1
chip clock = 124
chip power off gpio = 255
chip usb2 = 1
chip mode = 1
chip update = 0
chip udisk update = 0
chip select number = 1
chip select nand2 = 1
chip select nand3 = 1
chip select gpio = 0
chip gpio_pin = 254

wait time = 30
burned mode = 1
burned gpio = 1, 254, 1, 0, 255
burned rtc = 1, 1

cmdline support = 1
cmdline address = 0x0
cmdline data = 

ram type = 1
ram size = 16
ram row = 12
ram column = 9
ram bank = 4

mac start high = 01:02:03
mac start low = 00:00:00
mac end high = 01:02:03
mac end low = FF:FF:FF
mac addr flag = 0
fore write mac addr = 0

serial start high = AABBCCXXDD
serial start low = 000000
serial end high = AABBCCXXDD
serial end low = 999999
serial addr flag = 0
fore write serial addr = 0

online make image = 0

moduleburn DownloadMode = 0
moduleburn bDownloadFLS = 0
moduleburn bDownloadEEP = 0
moduleburn baudrate = 921600
moduleburn gpio_dtr = 85
moduleburn gpio_module_igt = 109
moduleburn gpio_module_reset = 87
moduleburn path_fls = LCG2.fls
moduleburn path_eep = LCG2.eep

fs reserver block = 64
fs nonfs reserve size = 4

partition count = 5
	partition1 = C, 0, 0, 0, 20
	partition2 = D, 0, 0, 0, 20
	partition3 = A, 0, 0, 0, 10
	partition4 = E, 0, 0, 0, 10
	partition5 = B, 1, 0, 0, 4000

volume lable count = 5
volume lable1 =  
volume lable2 =  
volume lable3 =  
volume lable4 =  
volume lable5 =  

download_to_udisk count = 0

download_to_nand count = 6
download_to_nand1 = 0, Sword37.bin, 0x30000000, BIOS
download_to_nand2 = 0, AkResData.Bin, 0x30500000, RES
download_to_nand3 = 1, E_0.wav, 0x0, E_0.wav
download_to_nand4 = 1, E_4.wav, 0x0, E_4.wav
download_to_nand5 = 1, beep.wav, 0x0, beep.wav
download_to_nand6 = 1, bell01.wav, 0x0, bell01.wav

download_to_mtd count = 0

nand supported count = 0

sflash supported count = 10
sflash 1 = 0x1640ef, 4194304,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 2 = 0x1640c8, 4194304,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 3 = 0x1530ef, 1048576,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 4 = 0x1540c8, 1048576,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 5 = 0x1440ef, 1048576,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 6 = 0x1630d5, 4194304,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 7 = 0x1740ef, 8388608,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 8 = 0x1740c8, 8388608,  256, 256, 65536, 30000000, 0x0, 0x0, 0
sflash 9 = 0x1740c8, 8388608,  256, 256, 65536, 30000000, 0x0, 0x0, 00
sflash10 = 0x1520c2, 4194304,  256, 256, 65536, 30000000, 0x0, 0x0, 000
